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[bookmark: _Hlk2275571][bookmark: _Hlk2326377]1 Description
Code : 	1-INT-GTV-BP6
Description :	Master interface for GTV62 1R
Gerber file :	1-INT-GTV-BP6 (gerber).zip
Component list:	1-INT-GTV-BP6 (component).xlsx
PCB Thickness	1.2 mm
PCB protection	conformal coating
PCB dimension	44 x 133.2 mm
Packing :	None
Label :	None
Multiple packaging :	Carton box




[bookmark: _Hlk2326418]2 Finish product

	Top	Bottom	
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3 Color led Switch
      
 The "int" switch allows you to select the desired LED lighting (blue or white) 
Default ON : blue color


[image: ]














      
4 PCB 


PCB Thickness	1.2 mm
PCB protection	conformal coating
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5 PIN
Characteristics
Supplier :	HARWIN
Description :	Male SIL Horizontal Throughboard Conn
Code  :	M20-9963645 
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Dimension in mm			Soldering detail 

6 WIRES (2)

Characteristics
- Conductor material 	Tinned annealed copper
- Type of conductor 	Circular, stranded 
- Insulation 	PVC 
- Outer sheath 	Unsheathed
- Cable flexibility 	Flexible
- Number of cores 	1
- Conductor cross section (AWG)	AWG24 (0.2mm²)
- Number of core wires (nb x mm Ø): 	7 x 32AWG 
- Connector (NEW):                                CN6	

Details

- Length:	40 cm (16 in)
- Color: 	Wire 1 (BP:0): Green 
	Wire 2: (BP 1): Red 
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7 COMPONENT LIST

Component list:	1-INT-GTV-BP6 (component).xlsx
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IMPORTANT
R
esistance R1 to R
4
 must have a tolerance of 1%
)
    




8 SCHEMATIC
Schematic :	1-INT-GTV-BP6 (schematic).jpg

[image: ]





image3.jpg
sures | S

Activate blue LEDs

Activate white LEDs




image4.JPG
1.2mm

Thickness




image5.emf

image6.emf

image7.jpg
Red Wire
16in (40cm)j

Green Wire
16in (40cm)




image8.jpeg




image9.jpeg




image10.JPG
list of components for PCB: 1-INT-GTV-BP6
Toiérankd Type KA Case sizdhd Suppiier K

a1 I 1870 ohms T sMD [T toTerance Cormector W
R Resistor 2320 onms % sMp 2fimperative tolerance 1% | | Diode 4
s Resistor 290 ohms % swp ~ ifimperative toterance 1% | | Resistor 4
3 Resistor 5740 onms % swp ~ tfimperative toterance 1% | | Transistor s
o7 Diode  PMLLALAEL SMD 1 | (vide)
£ PMLLeLdEL £ 1 Diode LED 6
) MiLs108L £ a Reduire 1
o1 BT — ET) 1 Green Wire 1
01 |Diode LED TF-S3527BW-DGYKLS £ OGIAED 1 Suitch 1
02 |Dioge LED T)-S3527BW-DGYELS £ ToGIALED | 1 Cortact C1B 2
D lode LED TH-S3527BW-DGYKLS £ TOGIALED 1 | Total général ©
0 Diode LED T1-S3527BW-DGYKLS £ ToGIALED | 1 |
05 Diode LED TJ-S3527BW-DGYKLS £ TOGIALED 1 |
06 Diode LED T1-S3527BW-DGYKLS £ TOGIALED | 1
a Transistor POTALZSIT 1
Transistor PDTALZ3IT 1
Transistor PDTALZAIT 1 [ 1
Transistor PDTALZ3IT 1
Transistor PDTCL2AIT 1 i
Transistor PDTCL2AIT - |
Transistor_PDTCL2AIT 1 I
Transistor PDTCL2AIT 1
[Transistor _pDTC123IT a
[connector_B128-Pr-ks 1
|Connector FARWIN 1
Connector RARWIN |1
Connector_ M20-9963645(1pin) HARWIN 1 i
Connector | M20-9963645(1pim) rARWIN 1 |
M20-996364511pin) HARWIN 1 |
Connector | M20-9963645(1pin) rARWIN |1
|connector 20996 n) HARWIN 1
Connector | M20-9963645(1pim) ARWIN 1
Connector_ M20-9963645(1pin) HARWIN 1
Connector s HAR 1
Connector M20-9963645(1pin) HARWIN 1 i
Connector | M20-9963645(1pin) HARWIN 1 |
0cm (1575inen) 1 I
Green wire 40cm (1575inch) 1
Swien ET) NIDEC a
Connecto TRAD s 1
i3 2
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